Lab1: Hello World

# 1 Objective

To become familiar with the basics: text editor, assembler, linker, and debugger. After finishing this experiment, you should be able to do the following:

1. Use a text editor to create an assembly source code (.s).
2. Understand the general procedure to develop and debug an assembly program.

# 2 Background

## 2.1 Assembler

In the following, we assume you have created aliases, e.g., “as32” for arm-linux-gnueabihf-as32, and “ld32” for arm-linux-gnueabihf-ld32.

To assemble a program (assuming the file name is lab1.s), one should type the command line:

$ as32 -g -o lab1 . o lab1 . s

where .s file is the source file and .o file is the output object file containing the machine code. We include debugging information by using -g.

## 2.2 Linker

The linker creates an executable file (or a library) from one or more object files:

$ ld32 −o lab1 lab1 . o

To run the program:

$ ./ lab1

The entry point of an assembly source program is usually referred to as32 “\_start”. If necessary, we can change the entry point to “main”:

$ ld32 −e main −o lab1 lab1 . o

As32 before, the linker will generate an executable file named “lab1”.

## 2.3 Debugger

The GNU debugger (**gdb**) allows you to execute, trace, inspect, and change variables during program execution. GNU DDD is a graphical front-end for command-line **gdb** debuggers.

# 3 Laboratory Workflow

## Part 1: “Hello World” Program

In this section you will create an assembly program that calls the “printf” function from the C runtime library.

1. Create a file named lab1p1.s by copying its content from the Appendix. You can use vim or some other text editor.
2. Assemble and link the files.

$ as32 -o lab1p1.o lab1p1.s

$ ld32 -o lab1p1 lab1p1.o

1. Execute the program by typing ./lab1p1. You should see the output“Hello World!”.

Next, run lab1p2.s, which implements the “printf” function from the C library in Assembly. You should see similar output as32 lab1p1.s.

## Part 3: Use the command-line tool gdb for debugging

In this section, we will use gdb to debug the **lab1p2.s** program.

In C programming, you can print out the value of each variable to make sure your program is functioning properly. In assembly, the **registers** take the position of “variables”, and you can examine their values with a debugger.


1. To start the debugger:

$ gdb lab1p2


You should see the following message on your screen.




1. Start the debug procedure by typing “**start**” within gdb:




1. Next, we use the command “**disassemble**”. There is an arrow =>pointing to the next instruction to be run.



1. Before running the program, let’s inspect some register values by using the “**info**” command.



1. To step into each instruction one by one, we use the “**stepi**” command. Then we can follow with another “**disassemble**” to see what has happened.



1. Repeat Steps 3˜5 and fill the table with register values after each instruction has been run.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | R0 | R1 | R2 | R7 |
| MOV R0,#1 |  |  |  |  |
| LDR R1, =message |  |  |  |  |
| MOV R2, =length |  |  |  |  |
| MOV R7, #4 |  |  |  |  |
| MOV R2, #3 |  |  |  |  |
| SWI 0 |  |  |  |  |
| MOV R7, #1 |  |  |  |  |
| SWI 0 |  |  |  |  |

Table 1: Instruction trace table.

**Lab deliverable 1**

Include Table 1 above in your lab report.




Figure 1: The DDD debugger.

## Part 3: Use the graphical interface DDD for debugging

In this section, we will use DDD to debug the **lab1p2.s** program. Enter the command:

$ ddd lab1p2

Under the “**View**” tab, open the “**Machine Code Table**”. Under the “**Status**” tab, click “**Registers**”. Now your interface should look similar to Figure 1. You can set a breakpoint by clicking in the blank area (left side as32 shown in Figure 1) next to each instruction.

Once the breakpoint has been set, click the “**Run**” button to start debugging and the “**stepi**” button to trace each instruction. The value of each register should be displayed in the Registers status window on the right side.

**Lab deliverable 2**

**lab1p2.s** contains a small bug. After fixing the bug, change the program to print your name before Hello World, e.g., “John Doe Hello World!”. Include the modified program in your lab report, and also upload it as a separate .s file on Canvas for execution and grading.

# 5 Report

Please use the project report template. Describe your experiences in completing the project, and make sure to include Lab deliverables 1 and 2.

# 6 Appendix

**lab1p1.s**

.data

message: .ascii "Hello World!\n"

.text

.global main

main:

push {ip, lr}

ldr r0, =message @ Load the starting address of the message

bl printf @ Call the printf function

mov r0, #0 @ Return 0.

pop {ip, pc}

**lab1p2.s**

.data

message: .ascii "Hello World!\n"

length = . – message @ Returns string length of message

.text

.global main

main:

@ write syscall

mov r0, #1 @ For stdout

ldr r1, =message @ buffer is loaded with message

ldr r2, =length @ count is the length of message

mov r7, #4 @ write is syscall 4

mov r2, #3

swi 0 @ interrupt

@ exit syscall

mov r7, #1

swi 0